C153

TB.e,TB,N-Well,"TO is not allowed to placed ,  if the space between two NW less than 0.96um  ",Spacing,<,0.96

应该是restrict

A1.a,A1,Metal 1,Min A1 width must be  >= 0.194um  ,Width,>=,0.194

A1.b,A1,Metal 1,Min A1 space must be  >= 0.194um  ,Spacing,>=,0.194

A1.e,A1,Metal 1,Minimum space between M1 lines with one or both metal line width  and length are greater than 10um is 0.476um  The minimum space must be maintained between a metal line and a  small piece of metal( < 10) that is connected to the wide metal  within 1.0um range from the wide metal  ,Spacing,>=,0.476

A1.g,A1,Metal 1,Min A1 area must be  >= 0.2um2  ,Area,>=,0.2

缺cdf